BL51 BANKED LINKER/LOCATER V6.05                                                        04/26/2015  23:45:35  PAGE 1


BL51 BANKED LINKER/LOCATER V6.05, INVOKED BY:
C:\KEIL\C51\BIN\BL51.EXE led.obj TO led RAMSIZE (256)


MEMORY MODEL: SMALL


INPUT MODULES INCLUDED:
  led.obj (LED)
  C:\KEIL\C51\LIB\C51S.LIB (?C_STARTUP)


LINK MAP OF MODULE:  led (LED)


            TYPE    BASE      LENGTH    RELOCATION   SEGMENT NAME
            -----------------------------------------------------

            * * * * * * *   D A T A   M E M O R Y   * * * * * * *
            REG     0000H     0008H     ABSOLUTE     "REG BANK 0"
            IDATA   0008H     0001H     UNIT         ?STACK

            * * * * * * *   C O D E   M E M O R Y   * * * * * * *
            CODE    0000H     0003H     ABSOLUTE     
            CODE    0003H     001DH     UNIT         ?PR?MAIN?LED
            CODE    0020H     000EH     UNIT         ?PR?_DELAY?LED
            CODE    002EH     000CH     UNIT         ?C_C51STARTUP



OVERLAY MAP OF MODULE:   led (LED)


SEGMENT
  +--> CALLED SEGMENT
---------------------
?C_C51STARTUP
  +--> ?PR?MAIN?LED

?PR?MAIN?LED
  +--> ?PR?_DELAY?LED



SYMBOL TABLE OF MODULE:  led (LED)

  VALUE           TYPE          NAME
  ----------------------------------

  -------         MODULE        LED
  C:0000H         SYMBOL        _ICE_DUMMY_
  D:0090H         PUBLIC        P1
  D:00B0H         PUBLIC        P3
  D:00A8H         PUBLIC        IE
  C:0020H         PUBLIC        _delay
  D:00B8H         PUBLIC        IP
  C:0003H         PUBLIC        main
  D:0098H         PUBLIC        SCON
BL51 BANKED LINKER/LOCATER V6.05                                                      04/26/2015  23:45:35  PAGE 2


  D:0088H         PUBLIC        TCON
  D:00C8H         PUBLIC        T2CON
  D:00D0H         PUBLIC        PSW
  -------         PROC          _DELAY
  D:0007H         SYMBOL        i
  -------         DO            
  D:0007H         SYMBOL        m
  D:0006H         SYMBOL        n
  -------         ENDDO         
  C:0020H         LINE#         19
  C:0020H         LINE#         20
  C:0020H         LINE#         22
  C:0026H         LINE#         23
  C:002DH         LINE#         24
  -------         ENDPROC       _DELAY
  -------         PROC          MAIN
  -------         DO            
  D:0005H         SYMBOL        k
  -------         ENDDO         
  C:0003H         LINE#         26
  C:0003H         LINE#         27
  C:0003H         LINE#         28
  C:0003H         LINE#         29
  C:0003H         LINE#         30
  C:0006H         LINE#         31
  C:0008H         LINE#         32
  C:0008H         LINE#         33
  C:000DH         LINE#         34
  C:001AH         LINE#         35
  -------         ENDPROC       MAIN
  -------         ENDMOD        LED

Program Size: data=9.0 xdata=0 code=58
LINK/LOCATE RUN COMPLETE.  0 WARNING(S),  0 ERROR(S)
